***RESUME***

**POST APPLIED FOR FLOORMAN**

**Mob - +91 9828013121**

**PERSONAL DETAILS**

**NAME** : BAJRANG SINGH RATHORE

**FATHER ‘S NAME** : UMMED SINGH RATHORE

**DATE OF BIRTH** : 15 JULY 1989

**WEIGHT** : 65

**HIGHT**  : 5’7”

**LANGUAGES KNOWS** : ENGLISH & HINDI

**PASSPORT** : L9747226

 ISSUED PLACE: JAIPUR, RAJSATHAN

**EDUCATION QUALIFICATION**: HIGH SCHOOL AT AJMER BOARD

**S.T.C.W COURSES&BOSIET (OPPITO APPROVED) AND H2S&BA**

* PST
* Fire Fighting
* HUET
* First Aid

 **EXPERIENCE & DETAILS**

|  |  |  |  |
| --- | --- | --- | --- |
| **Name of the Company** | **Position** | **Place** | **Duration** |
| **ABAN SINGAPOORE PRIVATE LIMITED** | **FLOORMAN** | **DUBAI** | **03 JAN 2017 TO TILL NOW** |
| NATIONAL DRILLING COMPANY |  FLOORMAN | ABUDHABI | 20 JUNE 2015 TO 10 AUG 2016 |
| JAGSSON INTERNATIONAL LIMITED | FLOORMAN | MUMBAI HIGH( INDIA ) | NOV 2013 TO MARCH 2015 |
| SHIVANI OIL&GAS EXPLORATION SERVICES | FLOORMAN | INDIA | SEP 2012 TO OCT 2013 |
| JOHAN ENERGY | ROUSTABOUT | INDIA | JULY 2010 TO JULY 2012 |

**WORK PROFILE:-**

* Checking the Drilling Equipment such as Tongs, Spinner, iron roughneck, slips, Dog clamp, safety pin and die.
* Changing the die if it is not proper.
* Checking FOSV safety valve.
* Using manual tong, HT100, HT65, proper greasing.
* Running the drill pipe by using the makeup tong upside and breakup tong tool joint downside.
* Pulling out the drill pipe by using the breakup tong upside and makeup tong tool joint downside and also using the spinner and mud bucket.
* Draw works in reverse for slip and cut.
* Handling the cashing: - 30 inch conductor cashing, as well as 20 inch, 13 3/8, 9 5/8, 7” Liner and also tubing job.
* Top drive greasing: - Use the man rider belt, Jerry biker and grease gun.
* Bop work: - Changing the pipe rams.
* Housekeeping in the Rig floor Drilling Equipment in proper place.
* Relieving the derrick man and working in derrick.
* Pump room: - Changing fault piston, swap sub rod, changing cooling water.

Pump room stand pipe lineup. Pit to pit circulation, lineup the jetting line and mixing lineup.

* Pit cleaning, the suction strainer, and discharge strainer if it is become fault.
* Co-ordinates with all co-workers and giving open hands to those who need help.

**ATTITUDES & ATTRIBUTES:-**

* Hard working, honest & dependable
* Successful, positive attitude
* Keen to accept responsibility
* Forward thinking attitude
* Strong self-discipline with attention to detail
* Self-starter and extremely motivated
* Achievement oriented and flexible

Email id : rathorebs1989@gmail.com

Date : 13\05\2017

Place : Nagaur

 Signature

 Bajrang Singh Rathore

 +91 9828013121